**COLLISION**

**-LIFEVESTS**

**-Where was the boat struck??**

**-Check the bilge for Water**

**IF WATER COMING IN, LOCATE DAMAGE!**

**-make sure that the bilge pumps are clear and pumping. Put crew on manual pump in Cockpit**

**-Start engine to charge batteries**

**Tools-**

**Collision Mat, Truplugs, cushions, axe, headlamps, crowbar**

**Repairs-**

**Underwater epoxy, fiberglass (mat and fibers), resin and hardener, self-tapping screws, plywood (seat in forward cabin), cordless drill.**